# Introduction

Biometric authentication systems is based on person’s anatomical features (fingerprints, face, palm veins, hand geometry, iris, voice) or behavioral traits (signatures, gaits, etc). Because these traits are physically user related, biometric authentication is one of the most reliable authentication systems. One of the perspective types of biometrics recently has proved to be electroencephalogram (EEG), since EEG signal is hard to fake because of the way EEG is being recorded.

In the last 20 years, in numerous studies different approaches of using EEG data as biometrics for identification [1]–[6] or authentication [7]–[11] of the subjects were proposed. The main difference between a system for authentication and identification is that the first require only verifying the identity, i.e confirming, that captured biometric data of the subject corresponds to the template of proposed identity, and therefore a task of binary classification in such system is presumed. At the same time, in identification system the goal is to recognize the person from some the data set of subjects, so multiclass classification in such system is presumed.

It is obvious that the identification approach would be too complex to use in a real-world system with a lot of users for authentication purposes. First of all, it narrows the opportunities of using such technologies of machine learning as neural networks, since multiclass classification increases the computational cost, while performing the worse results than binary classification. It was proven in [10] that identification system performs lower accuracy than authentication system, even though the same input data was used. Moreover, proposed identification systems were not intended for adding new users easily to the system, since it would require to change an output of the whole system and retrain it from scratch.

Therefore, in our work an authentication system based on EEG was proposed, since it is more rational approach that proved to be more accurate than identification when using the EEG data.

In the studies,3 types of stimulus were used for classifying the subject: rest state[1], [2], [6], [7], [12], Visual Evoked Potential [4], [11] and imaginary activity [3], [8], [10]. It is well known that authentication require the more consistent data, and in works [ citations, looks for proofs, ask Arno and Flavio] it has been proven that one of the most consistent types of recorded EEG data is recordings during motor activity. However, none of the aforementioned works used it as input data. Therefore, we proposed to use motor activity stimulus in order to achieve better accuracy and create more reliable system in terms of consistency of the input data.

Another problem in building authentication system is that the most appropriate channels and features for the authentication has not been distinguished yet. Therefore, one of the methods of avoiding leaving the information that could be important is to use all channels and as much as possible features. As long as neural network has proven to deal with classifying a high dimensional data with a high accuracy and low computational cost (comparing to other machine learning algorithms) [10][11], in this work it was proposed to use it as a classifier.

Moreover, in a lot of studies (for example [13], [14]), a method of improving the accuracy of classification by using the combination of neural network and Support Vector Machine (SVM) was proposed. In this works, neural network was used for convoluting the input into smaller number of feature vectors, and then this vector was fed into SVM for further classification. Thus, this method was used in our work as well.

As it was mentioned before, it is hard to distinguish the best channels. A Principal Component Analysis (PCA), as well as neural network, could be used for convoluting correlated set of variables into the new, smaller set of variables [15]. Therefore, in this work a PCA was used for convolution of the input data as well with the subsequent SVM for classification.

# 2. Materials and Methods

## 2.1 Materials

### 2.1.1 EEG recording

EEG dataset “EEG Motor Movement/Imagery Dataset”[16] was used from PhysioNet databank[17]. In this dataset subjects performed different motor/imagery tasks (in our work, only motor tasks were used) while 64-channel EEG was recorded using the BCI2000 system [18]. In total data from 105 subjects was used, each subject has around 25 trials (variate from 22 to 26). Each subject performed two one-minute baseline runs (one with eyes open, one with eyes closed) before all trials. For authentication, the following tasks were used: a target appears on either the left or the right side of the screen. The subject opens and closes the corresponding fist until the target disappears. Then the subject relaxes.

### 2.1.2 EEG preprocessing

Data was imported into MATLAB for analysis using custom-written scripts. The duration of the experiment excluding electrode setup was around 30 min. In total, for each subject around 25 trials for each task were used.  Before each trial there were 3-4 sec recording of relaxation, which then was used as a baseline. The EEG signal then was filtered using zero phase delay with range 1-50 Hz.

## 2.2 Feature Extraction Methods

### 2.2.1 EEG Spectral Analysis

Power Spectral Density (PSD) was calculated with multitaper method on Chronux toolbox[19]. For each channel 20 frequency bands were chosen from 1 to 40 Hz in log scale, and PSD was extracted.

### 2.2.2 EEG signal univariate complexity analysis

One of the methods of a signal representation is Empirical Mode Decomposition (EMD)[20]. This method represents a signal as a sum of modulated components known as IMFs.

Signal = IMF1 + IMF2 + IMF3 + ··· + IMFn

Each IMF connected with width of a frequency band: width gradually decrease with increasing of IMF number. The first IMF is calculated as mean signal between two signals, which created from local minimums and local maximums of the signal (figure 1). The next IMF is created with the same method, but using previous IMF as input.




Figure 1: Empirical Mode Decomposition method visualization

For each trial EMD was made with 40 dB resolution and 60 dB residual energy, and only first 5 intrinsic mode functions (IMFs) were left, as the most informative.

For each channel and for each first 5 IMFs the following entropies was obtained: Univariate Shannon entropy, log entropy, Sample entropy, Approximate entropy.

Shannon entropy *H*  [21] is given by the formula:

Log energy *H* [22] is given by the formula:

Where *p(x)* is the probability of character number *x* appearing in the stream of characters of the message.

Approximate entropy (ApEn)[23] is given by the formula:

Sample entropy (SampEn) [24]is given by the formula:

Bm –probability the similarity between 2 sequences with length m obeys r (tolerance level).

Am+1 –probability the similarity between the same 2 sequences with length m+1 obeys r.

The calculation of ApEn also includes self matches, while SampEn does not. In our work, m=2 and r was set as 15% of standard deviation of time-series.

## 2.3 Multivariate analyses methods

After feature extraction,40 features for each of 64 channels was gotten, from which matrix 40\*64 for each trial was formed. An obvious challenge was to reduce the size of the matrix to be able to use such machine learning techniques as SVM, and, what is more important, to investigate which of extracted features had the greatest significance in the problem of subjects authentication.

For this purposes, simultaneous multichannel analyses was proposed. It was found that within the same features between the channels there can be a connection, and the orders of values coincide within the characteristics, however, they can differ significantly between different features.


Based on cross-correlation method[25], 2 clusters of channels could be distinguished. Figure 2 represents mean cross-correlation of all characteristics. Therefore, the main idea was to do the convolution of the channels within each characteristic, after which 40\*2 matrix was gotten for each trial. Additionally, matrix 40\*1 was checked, but low accuracy of the system was performed in this case.

Figure 2: mean cross-correlation of all characteristics

### 2.3.1 Neural network horizontal convolution

Neural network[26] is one of the artificial intelligence algorithms, which was modeled on the principle of biological neural networks functioning, and could be used for pattern recognition, discriminant analysis or clustering. Moreover, neural networks could be used to compress big-scaled data into the smaller set of features, which later can be used in other classification methods. Therefore, in proposed systems neural network was used as a first part of larger machine-learning system in order to do the convolution between channels.

The main idea was to use a set of convolutional layers to find dependencies only within the characteristics (within rows), while not affecting the dependencies between the various characteristics (between columns); that is why in the convolutional layers only 1\*n-type filters where used.

For this purposes, the neural network was built using Keras framework in Python. Its model was based on the part of  “InceptionV3” model [27], the main feature of which is that it has filters of several sizes working at the same level, and had the following structure (figure 3).


Subsequently, the matrix 40 \* 64 was converted by this neural network into a matrix 40 \* 2. Then this vector was transformed into 80\*1 for SVM.

Figure 3: neural network structure

### 2.3.2 PCA


 Principal component analysis (PCA)[28] is a mathematical procedure that transforms a number of possibly correlated variables into a smaller number of uncorrelated variables called principal components (Figure 4)[15].

Figure 4: PCA method visualization

In this work, our convolution method was compared with the common one, that is why matrix 40 \* 64 was converted by PCA into a matrix 40 \* 2, like NN does. Then this vector was transformed into 80\*1 for SVM.

## 2.4 Classification method

### 2.4.1 Build classification model

Three authentication systems were built: in the first system, the input data was opening and closing of the left fist, in the second - opening and closing of the right fist, and input data for the third system was a sequence of two actions (compression of the left and right fist). In the third system, the subject passed authentication only in the case of correct prediction of each actions, which was done in order to reduce the type II error. For each system, 3 different models were applied.

In the first model (NN model), aforementioned NN, that was expanded with the set of Dense layers, was used for authentication.

In the second model (NN+SVM model), the combination of pre-trained neural network and SVM was used. Thus, at first horizontal convolution of matrix was done using NN, and then this data was given as input into SVM for final classification.

In the third model (PCA+SVM model), horizontal convolution was performed using PCA, and then this data was classified via SVM as in the NN+SVM system.


For training model for one user was used a sample, which included 22 recordings from a given subject, and 28 recordings from other users, selected as follows: for all registered in the system users, 28 users were randomly selected, and for each of them one EEG recording was randomly selected as well.

Figure 5: explanation of NN model, NN+SVM model, and PCA model

### 2.4.2 Training neural network for NN and NN+SVM models


For classification, as well as for training the layers of model of neural network, presented in the chapter 2.3.1, the aforementioned model was expanded with the set of Dense layers. Moreover, a Dropout layer was added in the middle of this set for reducing overfitting of network. The structure is presented in the figure 6. For training, Adam optimization method[29] was used with learning rate 10-4.

Figure 6: Set of layers, by which NN was expanded

### 2.4.3 SVM

Input for SVM could be from PCA or from NN. The main plus of SVM is the fast speed, that is why it is possible to choose the best group of features with method known as a grid selection.

#### 2.4.3.1 Grid selection

Accuracy of classification was compared, which was obtained from 5 fold cross validation for each feature, and then feature with the biggest accuracy was left. After that for all possible pairs (first best features and all other ones) accuracy was calculated as well, and best pair was chosen (figure 7).


Then best groups of features was compared for different subject and for different decompositions.

Figure 7: Grid selection method visualisation

# 3. Results and discussions

## 3.1 Obtained accuracy of the system

To obtain the accuracy of the model, 5-fold cross-validation method was used. Inside each fold, the training data was normalized inside each characteristic, and then the model was trained in a training sample and tested on a test sample, which was normalized using the minimum and maximum values of the training sample.


Roc-curves of all models are presented at Figure 8-10 for the systems, based on right, left and both fists respectively.

Figure 8: ROC for T1





Figure 10: ROC for both

Figure 9: ROC for T2

Accuracy and error Type I, II was calculated for all models and all systems and presented at Table 1-3.

As long as the wrong person should never be authenticated, Type II error is the most important for authentication system, and should be as low as possible.

Table 1: accuracy of NN model

Table 2: accuracy of PCA+SVM model

|  |  |  |  |
| --- | --- | --- | --- |
|  | **Right fist** | **Left fist** | **Both fists** |
| Type I error | 0.0251 | 0.0265 | 0.0482 |
| Type II error | 0.0095 | 0.0097 | 0.0011 |
| Overall accuracy | 0.9653 | 0.9638 | 0.9507 |

|  |  |  |  |
| --- | --- | --- | --- |
|  | **Right fist** | **Left fist** | **Both fists** |
| Type I error | 0.1272 | 0.1136 | 0.2272 |
| Type II error | 0.0999 | 0.1035 | 0.0178 |
| Overall accuracy | 0.888 | 0.892 | 0.89 |

Table 3: accuracy of NN+SVM model

|  |  |  |  |
| --- | --- | --- | --- |
|  | **Right fist** | **Left fist** | **Both fists** |
| Type I error | 0.0200 | 0.0500 | 0.0700 |
| Type II error | 0.0120 | 0.0400 | 0.0040 |
| Overall accuracy | 0.9680 | 0.9100 | 0.9260 |

## 3.2 Best features

As a result of grid selection method, the following features were returned as the best for authentication in PCA+SVM system:

* For right fist: Shannon entropy, Approximate entropy
* For left fist: Shannon entropy, Approximate entropy, log energy entropy.

At the same time, for NN+SVM model, the following results were obtained:

* For right fist: osculation in delta and beta rhythm, Approximate entropy, log energy entropy.
* For left fist: osculation in delta and beta rhythm osculation, log energy entropy, Approximate entropy.

# List of reference:

[1] A. Riera, A. Riera, A. Soria-frisch, M. Caparrini, I. Cester, and G. Ruffini, “1 Multimodal Physiological <em>Biometrics</em> Authentication.”

[2] R. B. Paranjape, J. Mahovsky, L. Benedicenti, and Z. Koles, “The electroencephalogram as a biometric,” *Can. Conf. Electr. Comput. Eng.*, vol. 2, pp. 1363–1366, 2001.

[3] Shiliang Sun, “Multitask learning for EEG-based biometrics,” pp. 1–4, 2009.

[4] R. Palaniappan, “Method of identifying individuals using VEP signals and neural network,” *IEE Proc. - Sci. Meas. Technol.*, vol. 151, no. 1, pp. 16–20, Jan. 2004.

[5] P. Kumari Sharma and A. Vaish, “Individual identification based on neuro-signal using motor movement and imaginary cognitive process,” *Optik (Stuttg).*, vol. 127, no. 4, pp. 2143–2148, 2016.

[6] Q. Zhao *et al.*, “Improving Individual Identification in Security Check with an EEG Based Biometric Solution,” Springer, Berlin, Heidelberg, 2010, pp. 145–155.

[7] M. Poulos, M. Rangoussi, V. Chrissikopoulos, and A. Evangelou, “Parametric person identification from the EEG using computational geometry,” *Proc. IEEE Int. Conf. Electron. Circuits, Syst.*, vol. 2, no. 1, pp. 1005–1008, 1999.

[8] S. Marcel and J. R. Millan, “Person Authentication Using Brainwaves (EEG) and Maximum A Posteriori Model Adaptation,” *IEEE Trans. Pattern Anal. Mach. Intell.*, vol. 29, no. 4, pp. 743–752, Apr. 2007.

[9] S. K. Yeom, H. Il Suk, and S. W. Lee, “Person authentication from neural activity of face-specific visual self-representation,” *Pattern Recognit.*, vol. 46, no. 4, pp. 1159–1169, 2013.

[10] J. F. Hu, “New biometric approach based on motor imagery EEG signals,” *FBIE 2009 - 2009 Int. Conf. Futur. Biomed. Inf. Eng.*, pp. 94–97, 2009.

[11] Q. Wu, Y. Zeng, C. Zhang, L. Tong, and B. Yan, “An EEG-based person authentication system with open-set capability combining eye blinking signals,” *Sensors (Switzerland)*, vol. 18, no. 2, pp. 1–18, 2018.

[12] I. Nakanishi, “Personal Authentication Using New Feature Vector of Brain Wave Personal Authentication Using New Feature Vector of Brain Wave,” no. January, 2017.

[13] S. Kaur and E. D. Kaur, “HYBRID MODEL USING COMBINATION OF NEURAL NETWORK AND SUPPORT VECTOR MACHINE FOR DETECTION OF LUNG CANCER,” vol. 2, no. 2, pp. 39–42, 2015.

[14] Y. Cao, R. Xu, and T. Chen, “Combining Convolutional Neural Network and Support Vector Machine for Sentiment Classification,” Springer, Singapore, 2015, pp. 144–155.

[15] “Supervised Machine Learning — Dimensional Reduction and Principal Component Analysis.” [Online]. Available: https://hackernoon.com/supervised-machine-learning-dimensional-reduction-and-principal-component-analysis-614dec1f6b4c. [Accessed: 07-May-2019].

[16] G. Schalk, D. J. McFarland, T. Hinterberger, N. Birbaumer, and J. R. Wolpaw, “BCI2000: A General-Purpose Brain-Computer Interface (BCI) System,” *IEEE Trans. Biomed. Eng.*, vol. 51, no. 6, pp. 1034–1043, Jun. 2004.

[17] A. L. Goldberger *et al.*, “PhysioBank, PhysioToolkit, and PhysioNet,” *Circulation*, vol. 101, no. 23, Jun. 2000.

[18] “BCI2000 | Schalk Lab.” [Online]. Available: http://www.schalklab.org/research/bci2000. [Accessed: 07-May-2019].

[19] “Chronux Home.” [Online]. Available: http://chronux.org/. [Accessed: 07-May-2019].

[20] “Empirical Mode Decomposition: Riding the Waves.” [Online]. Available: http://brocabrain.blogspot.be/2011/04/empirical-mode-decomposition-riding.html. [Accessed: 10-May-2018].

[21] C. E. Shannon and W. Weaver, “THE MATHEMATICAL THEORY OF COMMUNICATION,” 1949.

[22] S. Aydın, H. M. Saraoğlu, and S. Kara, “Log Energy Entropy-Based EEG Classification with Multilayer Neural Networks in Seizure,” *Ann. Biomed. Eng.*, vol. 37, no. 12, pp. 2626–2630, Dec. 2009.

[23] S. M. Pincus, “Approximate entropy as a measure of system complexity.,” *Proc. Natl. Acad. Sci. U. S. A.*, vol. 88, no. 6, pp. 2297–301, Mar. 1991.

[24] J. S. Richman and J. R. Moorman, “Physiological time-series analysis using approximate entropy and sample entropy,” *Am. J. Physiol. Circ. Physiol.*, vol. 278, no. 6, pp. H2039–H2049, Jun. 2000.

[25] E. W. Weisstein, “Cross-Correlation.”

[26] M. H. Hassoun and M. H., *Fundamentals of artificial neural networks*. MIT Press, 1995.

[27] C. Szegedy, V. Vanhoucke, S. Ioffe, J. Shlens, and Z. Wojna, “Rethinking the Inception Architecture for Computer Vision,” Dec. 2015.

[28] H. Abdi and L. J. Williams, “Principal component analysis,” *Wiley Interdiscip. Rev. Comput. Stat.*, vol. 2, no. 4, pp. 433–459, Jul. 2010.

[29] D. P. Kingma and J. Ba, “Adam: A Method for Stochastic Optimization,” Dec. 2014.